wl fergel, TTSIe IH, (ThE SHEER [fen Fie wea AFIT AF Taam @Ie (ATE) | we

ST, Fie TH @ Twi
CE Gf | 2AfSHETBa Bleed Ad

(wfsfae wiry) fem area |

Firm srrTER

sizeof Safe (@fsfe
wiiferg) AT) 2iif Saw cae
(offen) |

ffi 2a = Ate
ABCA bf Faia 29 fi
GREET 24 (A052 | G1
RIT! fafa Ame
AIBLAITS AZRIR 2AEAT ACTH
Geli ATIC &% Sf 2055 €
205 ITA AIF Haze
FAG TT (US AG MT
13 | oq foe @i0z ow wk
2030 vile Ad Hie
ABLAICS SNE bisa 23

OIA 2S &F FA

wie #ifGrara frie Aq Es
2091 | 5% 2030 iF (4S
“AIT forers wgria fey
73rsl foe | Afra Zaz
73g PAGES | FEN 2
251 axel, «2 ATH dt
Sei els firs 7a, ¢1
TRIE ell (TIE (B31 FE
0 SE AAA GT
EAGT fice fe ore,
dre ols Seid fee 2
G13 Rife wl wz |

ATG 2
o ef: soo (ffs
q0+©(29| 90)
o faf¥s: 90 warms so+
ferAlars wie © fel
90 THE TATHHS AI], Rf,
IE GI (20 20% #0 |
rel Fife Fufmif smifde
fafen sagas «Is | Gis
WIRE SE oe afer Sem
SEEIES (OF Indiabix.com,
examveda.com Z@ilfir (40
fifea 2fufwife Ase
HAGHS (7409 20 | AH
11, Bt, Slee Sie ger
fafiarT dele 2 7Te 2@
as fafen viraifos awgrd
“51 FICE Sle] I 20 |

I Ty ROT! ISG FT RI Fre 2ST Gefad bifEt
ri eres fie Rife atenen Asm a-fefedme 2fgfmm

E 80 We FEB0rsm wid
© Fsfn ga oes ff afer
aire | aE WE FifeA
Ffeifemira, wre 712 Gif (4
Fifent lyfe Anh fen
ARE | 2% Fel 3
«2 Aibf feo JKT Water
Resource Engineering
TEBE FF Gg AI FS
A | GF BH (ACE Cf Wie
PICA | Water Resource
Engineering 904 SI07| 4%
i Fluid Mechanics, Open
Channel Flow, Hydrology «4s
Irrigation Engineering &
faze SitEl Sa ATES WY
A ATA G2 21 AA | Ze
«af 2% «=a SFD-BMD
0% | @ lel Fe Sree
(210% N14 WE FG lz —
© Influence line
© Beam Design
Punching Shear of Footing
© BOD-«7 wt
Column Design
® Active Pressure, Passive
Pressure-4% 371%
© Fineness Modulus-«% 71%
Zein
« gel FF Aes 2 ©
Pi fifa qraen Hews
oe Af 93 (ETB
face Qe a ffi)
https /t.lyloyiC @7tz7 25
Rl Ate Fafte «abl
Arell A1eT FE wa @ EF

ot ed
FAV Spel FTAA

08 A498 AF 2H ANG
a bref fie 23m
wage @ae bref
wae @M @I B09 CSI |
fae 3s Bet warm
WIE TIF! | ATrAS SiZeH
ow Fie AF WE AA
cf srg faf4e we Sil
204 (7 Bll 716¥1 CFE
HTD! «PIE «I |
2AITAICe ©iZe! @BHEG

1% 2% Si 2AfebitT
PEE | SIZES SICH FE
Gif Area FER SEs doe
fate gta —

Grea/AEg Ene age
fits (vga Fane
fe Sia, Best IE
(fbi raf saa GRE
areal, a ATs arte
512, Introduce yourself 42
> 2a Tag AA (A 5
«0a 141, Fes cm Fie
“rare ARS BiG, AS
se fewfes wit, ce —
Zerg ALi Fac,
2AeTE TN SB, FE FER
2ATrAle 2% Zoi,
AAS fi @ fourm, #iSearg
foam, yfeym, ag (14
yfgga wz FEE ge
Beilin)

frre

MY Ate EIR 2ASETS
Freie 5f (710s 2A Gi
FACE BIG 9a bl «rel
meu (31 Stafz| wea
fifen Safi am AS
bref cf SIE | Hie
wwe Fem fufmies gam
24, WA TEES 2) oF
fees wifes Safes on
AGA bial (4 Site | &wig
aifgqzs (4 SIEPiReTS
Fed] ACE FI Gen
2 AACS | 741 GT
GS |

«eiffel RACHA AZ

